Welded atintersection of angled anchorsand vertical anchor

39 3/8"( 1 m ) intersection height27 1/2"( 0.70 m )

35�TITLEDRAWINGNUMBERDATEDRAWNBYSCALEUniversity of CaliforniaIGPP 0225La Jolla, California 92093

DESIGNED BY: S. DockterPi�on Flat ObservatoryC B Hollinshead16 Sep 981"=15"MDR-130 Driven Rod Monument Complete Assy.

~ 30 ft.

~ 7 ft.

~ 7 ft

~30 ft1:1 Clay &Bentonite1:2:1Peralite,Sand & Grout

6"~6 ft

6"1:1 Clay &Bentonite

4 1/2"Doverdrill

Welded coupler(as needed)MDR-34-1

1" rods w/ one End RodMDR-32, one IntermediateRod MDR-33 w/ dimples, and as many more Intermediate Rods MDR-33as can be driven in each of5 locations. Driven rods joined with Stud Coupler MDR-34-2, and welded