TITLEDRAWINGNUMBERDATEDRAWNBYSCALEUniversity of CaliforniaIGPP 0225La Jolla, California 92093

Do Not Scale This DrawingPi�on Flat ObservatoryC B Hollinshead2 Oct 981"=12"MDA-30(’98) SurfaceAssemblyPlan

Welded atintersection of angled anchorsand vertical anchor

Gussetted with 1/4"steel triangles weldedbetween angled anchorsand vertical anchorSee Detail

Pipe clamp preventspipe from slippinginto casing beforepouring grout andwhile grout sets

Side View ofPipeclamp(angle iron and U-bolt)

75-3/4"

62" (1.57m)

43-1/2"

68-3/16"from topof pipeto clamp

Intersection height

3"2 5/16"

1 1/4"

1 1/2"Point ofIntersection

57-1/2"from top of pipeto clamp

35�Measure angledpipe lengthfrom this point

~6"12"Drilled and Braced Monument